**Non contact Voltage Tester**

SAPINENI JAYADEEP AM.SC.U4CSE24153

SARANG P AM.SC.U4CSE24154

SHIVA SOORYA SREEKUMAR AM.SC.U4CSE24155

**Introduction:**

To provide a quick and easy method for identifying the presence of voltage in electrical circuits, especially in hard-to-reach or dark space

**Methodology**:

A Non-Contact Voltage Tester works by detecting the electromagnetic field generated by AC voltage. When an AC current flows through a conductor, it creates a varying magnetic field around it. This tester detects that field without needing to make direct contact with the conductor.

**Result**:

* The project demonstrates that a functional voltage tester can be built using basic, inexpensive components.
* The device provides a reliable method to verify the absence of voltage before working on electrical systems, reducing the risk of electric shock.

**Conclusion:**

* The tester detects the presence of AC voltage without direct contact, ensuring user safety.
* The project offers valuable learning opportunities in electronics, particularly in understanding electromagnetic fields and transistor amplification

Circuit diagram :

